0. Building on *nix from git repository

    Run the autogen script to generate configure, then proceed to step 1.
    Prerequisites: You'll need autoconf, automake and libtool installed.

    $ ./autogen.sh

1. Building on *nix from a release

    $ ./configure
    $ make
    $ make check   # (optional, but highly recommended)
    $ sudo make install

2. Building on iOS

    Use on the xcode project in IDE/iOS/wolfssl.xcodeproj
    There is a README in IDE/iOS with more information

3. Building on Windows

    Use the 32bit Visual Studio Solution wolfssl.sln
    For a 64bit solution please use wolfssl64.sln

4. Building with IAR

    Please see the README in IDE/IAR-EWARM for detailed instructions

5. Building with Keil

    Please see the Keil Projects in IDE/MDK5-ARM/Projects

6. Building with Microchip tools

    Please see the README in mplabx

7. Building with Freescale MQX

    Please see the README in mqx

8. Building with Rowley CrossWorks for ARM

    Use the CrossWorks project in IDE/ROWLEY-CROSSWORKS-ARM/wolfssl.hzp
    There is a README.md in IDE/ROWLEY-CROSSWORKS-ARM with more information

9. Building with Arduino

    Use the script IDE/ARDUINO/wolfssl-arduino.sh to reformat the wolfSSL
    library for compatibility with the Arduino IDE. There is a README.md in
    IDE/ARDUINO for detailed instructions.

10. Porting to a new platform

    Please see section 2.4 in the manual:
    http://www.wolfssl.com/yaSSL/Docs-cyassl-manual-2-building-cyassl.html

